Invalid Run

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org

CINT2000 Result

Copyright ©1999-2000, Standard Performance Evaluation Corporation -- SPECint2000 = SPECint_base2000 =

2232 2110

SPEC license #:000407 Tested by: Vladimir Makarov Test date: Jul 07, 2021 Hardware Avail: Now Software Avail: Now

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

164.gzip 1400 96.4 1453 92.0 1522

175.vpr 1400 77.4 1810 75.8 1848

176.gcc 1100 41.6 2646 X X

181.mcf 1800 106 1693 107 1680

186.crafty 1000 40.7 2458 37.7 2652

197.parser 1800 133 1350 131 1374

252.eon 1300 49.9 2604 39.7 3273

253.perlbmk 1800 65.9 2731 65.7 2741

254.gap 1100 53.6 2051 52.3 2102

255.vortex 1900 70.0 2716 50.6 3755

256.bzip2 1500 81.0 1852 72.7 2064

300.twolf 3000 110 2723 110 2728

Hardware

CPU: Genuine Intel(R) CPU @ 2.66GHz CPU MHz: 2666.555 FPU: Integrated CPU(s) enabled: 4 CPU(s) orderable: Parallel: No Primary Cache:

Secondary Cache: 4096 KB L3 Cache: Other Cache:

Memory: 4036100 kB Disk Subsystem: Other Hardware:

Software

Operating System: Linux 5.1.16-200.fc29.x86_64 Compiler: gcc version 12.0.0 20210707 (experimental) (GCC) File System:

System State: multiuser

Notes/Tuning Information

 Base flags: -O2 -mtune=generic
 Peak flags: -Ofast -flto

Errors

’reportable’ flag not set during run 176.gcc peak did not have enough runs!