Invalid Run

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org

CFP2000 Result

Copyright ©1999-2000, Standard Performance Evaluation Corporation -- SPECfp2000 = SPECfp_base2000 =

2059 1727

SPEC license #:000407 Tested by: Vladimir Makarov Test date: Jun 17, 2021 Hardware Avail: Now Software Avail: Now

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 2000 4000 6000 8000

168.wupwise 1600 95.8 1670 76.3 2097

171.swim 3100 129 2402 138 2244

172.mgrid 1800 170 1059 147 1227

173.applu 2100 158 1329 162 1295

177.mesa 1400 116 1207 64.8 2161

178.galgel 2900 69.7 4162 62.0 4676

179.art 2600 42.5 6122 36.2 7183

183.equake 1300 63.1 2059 60.1 2162

187.facerec 1900 111 1708 65.7 2893

188.ammp 2200 150 1469 136 1612

189.lucas 2000 123 1621 106 1887

191.fma3d 2100 146 1438 123 1706

200.sixtrack 1100 154 716 113 970

301.apsi 2600 185 1404 181 1438

Hardware

CPU: Genuine Intel(R) CPU @ 2.66GHz CPU MHz: 2666.445 FPU: Integrated CPU(s) enabled: 4 CPU(s) orderable: Parallel: No Primary Cache:

Secondary Cache: 4096 KB L3 Cache: Other Cache:

Memory: 4036100 kB Disk Subsystem: Other Hardware:

Software

Operating System: Linux 5.1.16-200.fc29.x86_64 Compiler: gcc version 12.0.0 20210617 (experimental) (GCC) File System:

System State: multiuser

Notes/Tuning Information

 Base flags: -O2 -mtune=generic -m32
 Peak flags: -Ofast -flto -m32

Errors

’reportable’ flag not set during run