Invalid Run

Standard Performance Evaluation Corporation info@spec.org http://www.spec.org

CINT2000 Result

Copyright ©1999-2000, Standard Performance Evaluation Corporation -- SPECint2000 = SPECint_base2000 =

2294 2096

SPEC license #:000407 Tested by: Vladimir Makarov Test date: Jun 21, 2021 Hardware Avail: Now Software Avail: Now

Benchmark

Reference

Time

Base Runtime

Base Ratio Runtime Ratio 1000 2000 3000 4000

164.gzip 1400 97.9 1431 92.4 1515

175.vpr 1400 78.7 1778 73.2 1913

176.gcc 1100 40.2 2737 X X

181.mcf 1800 56.1 3209 61.9 2906

186.crafty 1000 52.2 1917 47.3 2114

197.parser 1800 113 1590 99.0 1818

252.eon 1300 74.3 1750 51.5 2525

253.perlbmk 1800 68.2 2638 62.7 2872

254.gap 1100 51.9 2119 50.6 2173

255.vortex 1900 79.4 2393 50.4 3770

256.bzip2 1500 89.8 1671 84.7 1771

300.twolf 3000 111 2698 110 2719

Hardware

CPU: Genuine Intel(R) CPU @ 2.66GHz CPU MHz: 2666.490 FPU: Integrated CPU(s) enabled: 4 CPU(s) orderable: Parallel: No Primary Cache:

Secondary Cache: 4096 KB L3 Cache: Other Cache:

Memory: 4036100 kB Disk Subsystem: Other Hardware:

Software

Operating System: Linux 5.1.16-200.fc29.x86_64 Compiler: gcc version 12.0.0 20210621 (experimental) (GCC) File System:

System State: multiuser

Notes/Tuning Information

 Base flags: -O2 -mtune=generic -m32
 Peak flags: -Ofast -flto -m32

Errors

’reportable’ flag not set during run 176.gcc peak did not have enough runs!